### For Windows XP

1In [Control Panel], click [Network and Internet Connections].

The [Network and Internet Connections] dialog box opens.

2Click [Network Connections].

The [Network Connections] dialog box opens.

Under [LAN or High-Speed Internet], the icon representing your LAN interface (Ethernet adapter) configuration appears.

3Right-click on the LAN interface (Ethernet adapter) configuration icon and click [Properties] in the context menu.

The [Local Area Connection Properties] dialog box opens, with the [General] tab shown.

4In the [This connection uses the following items:] list box, select the [Internet Protocol (TCP/IP)] check box.

Confirm that the [Internet Protocol (TCP/IP)] check box is selected. If deselected, select the check box.

5Click [Properties].

The [Internet Protocol (TCP/IP) Properties] dialog box opens, with the [General] tab shown.

6Select the [Use the following IP address:] radio button and specify the IP address, the subnet mask, and the default gateway.

7Check the configured settings and click OK.

You are now done with the TCP/IP configuration.

Close all the dialog boxes that are open.