### COutputting an alarm signal from alarm output terminal

Configure the output conditions for each alarm output terminal.

AConfiguring automatic alarm output: | Configure the terminal so that it outputs an alarm signal automatically when an alarm condition is detected.
BConfiguring remote alarm output: | Configure the terminal so that it outputs an alarm signal when the corresponding Remote Alarm button is clicked.

Before you start the following procedure, connect an external alarm device to one of the alarm output terminals (“ALARM OUT1” in this example).
For details, refer to the “Alarm Input/Output Terminal Connections” section.

#### AConfiguring Automatic Alarm Output

1In [ALARM OUT1], select “ON”.
2In [POLARITY], select the signal polarity of the alarm output terminal.

NO (Normally Open): | The terminal is normally open and closes when an alarm signal is output.
NC (Normally Closed): | The terminal is normally closed and opens when an alarm signal is output.

3In [ALARM OUT TIME], select how long you want the terminal to output an alarm signal.

The terminal will stop outputting the alarm signal when the set alarm output time expires.

2SEC, 5SEC, 10SEC, 15SEC, 30SEC, 45SEC, 1MIN, 2MIN, 3MIN, 4MIN, 5MIN

The alarm output time must be specified within the duration of the alarm input terminal you select under [TRIGGER].

4Under [TRIGGER], configure the following alarm output conditions and click SET.

###### ALARM IN

Specify the alarm input terminal to which the alarm input device is connected. The ALARM OUT 1 terminal outputs an alarm signal when this terminal receives an alarm signal.

ALARM IN1: | The terminal outputs an alarm signal when the ALARM IN1 terminal receives an alarm signal.
ALARM IN2: | The terminal outputs an alarm signal when the ALARM IN2 terminal receives an alarm signal.

###### MOTION

You can configure the alarm output conditions in conjunction with the motion alarm function.

OFF: | The terminal does not output an alarm signal even when motion is detected in the subject by the motion sensor.
ON: | The terminal outputs an alarm signal when motion is detected in the subject by the motion sensor.

* To configure the ALARM OUT 2 terminal to output an alarm signal, select “ON” in [ALARM OUT2] and specify the output conditions for it in the same way as for the ALARM OUT1 terminal.

#### BConfiguring Remote Alarm Output

1In [ALARM OUT1], select “REMOTE”.

Selecting “REMOTE” does not cause the terminal to output an alarm signal automatically even if an alarm condition is detected.

2In [POLARITY], select the signal polarity of the alarm output terminal.

NO (Normally Open): | The terminal is normally open and closes when an alarm signal is output.
NC (Normally Closed): | The terminal is normally closed and opens when an alarm signal is output.

3In [ALARM OUT TIME], select how long you want the terminal to output the alarm signal and click SET.

The terminal will stop outputting the alarm signal when the set alarm output time expires.

2SEC, 5SEC, 10SEC, 15SEC, 30SEC, 45SEC, 1MIN, 2MIN, 3MIN, 4MIN, 5MIN

CC (Stops outputting the alarm signal when the corresponding Remote Alarm button is clicked on the live screen.)

###### To configure the ALARM OUT 2 terminal to output an alarm signal when a Remote Alarm button is clicked, select “REMOTE” in [ALARM OUT2] and specify the output conditions for it in the same way as for the ALARM OUT1 terminal.