### MIRROR

Use the mirror function to electronically flip the displayed subject.

If you installed the camera upside down or intend to monitor the subject in the mirror, configure the following settings according to the installation environment of the camera.

###### In [MIRROR], select the desired mirror mode and click SET.

OFF: | Disables the mirror mode (normal video).
HV: | Flips the video vertically and horizontally.
H: | Flips the video horizontally.
V: | Flips the video vertically.

The configured settings will be applied commonly to “CAM1” and “CAM2” selected under [VIEW].