Click FTP in the configuration menu to display the FTP SETTINGS screen.

If you want to record images from the camera to an FTP server via the network, configure the FTP server settings and the image transmission conditions on this screen.

AConfiguring FTP server settings

BConfiguring transmission conditions

Required operation privilege: admin, operator

You can send JPEG images only.

### AConfiguring FTP Server Settings

1In [FTP], select “ON”.

2In [PORT NUMBER], type the control port number configured on the server.

Type a number between 1 and 65535. This port number is normally “21” (default).

3In [SERVER ADDRESS], type the server address. Then, in [USER ID] and [PASSWORD], type the user ID and password, respectively.

The number of characters you can type in these fields is as follows.

SERVER ADDRESS: Up to 64 alphanumeric characters

USER ID: Up to 48 alphanumeric characters

PASSWORD: Up to 20 alphanumeric characters

4To use the passive FTP mode, in [FTP PASSIVE], select “USE”.

When [FTP PASSIVE] is set to “USE”, users must specify a valid port number when making a connection request for sending data to the server.

5In [DIRECTORY NAME], specify the name of the directory you want to create on the server.

You can type up to 32 alphanumeric characters.

If no directory name is specified, the system will automatically generate the following directory name.

When sending an alarm image in the event of an error: ALARM_FTP

When sending an image in fixed intervals: INTERVAL_FTP

6In [FILE NAME], specify the name of the image file you want to send and click SET.

You can type up to 32 alphanumeric characters.

Each image file will have a file name consisting of the specified file name, the date/time, and the alarm factor (if [TRIGGER] is set to other than “INTERVAL”):
[FILE NAME] + [yy_mm_dd_hh_mm_ss] + [alarm_factor] + [0001 (Serial No.).jpg]

If no file name is specified, the system will enter “sanyo” for the [FILE NAME].

###### * To use a temporary file, set [TEMPORARY FILE] to “USE”.

This causes each image to be stored as a temporary file on the FTP server and then renamed to the specified file name.

The FTP server will store a single temporary file for the most recent image with the specified file name.

Temporary file name: sanyo_ftp_temp_[IP address].temp

Although the temporary file will be renamed to the specified file name and then stored in the specified directory as explained in steps 5 to 6, the renamed file name will not include the date/time and alarm factor information.

Both the temporary and permanent files will be overwritten if the same file name exists.

### BConfiguring transmission conditions

###### In [TRIGGER], select the image transmission trigger condition, configure items as necessary and click SET.

INTERVAL: Sends a still image in fixed intervals.

ALARM IN1: Sends a still image when the ALARM IN1 terminal receives an alarm signal.

ALARM IN2: Sends a still image when the ALARM IN2 terminal receives an alarm signal.

MOTION: Sends a still image when the motion sensor detects motion in the subject.

ALARM OUT1: Sends a still image when the ALARM OUT 1 terminal outputs an alarm signal.

ALARM OUT2: Sends a still image when the ALARM OUT 2 terminal outputs an alarm signal.

NETWORK FAILURE: Sends a still image when the camera detects a network failure during network recording.

You need to configure the alarm input/output conditions on the ALARM SETTINGS screen.

###### AIf you selected “NETWORK FAILURE” ...

In [NETWORK FAILURE TIME], select the time from the occurrence of a network failure until the camera recognizes it as a recording trigger.

15SEC, 20SEC, 30SEC, 40SEC, 50SEC, 1MIN, 2MIN, 3MIN, 4MIN, 5MIN

The setting values are interlocked among E-MAIL SETTINGS, and FTP SETTINGS screens. (Note that the setting configured most recently will take precedence.)

###### BIf you selected “ALARM IN1/2”, “MOTION”, or “ALARM OUT1/2” ...

In [DURATION], select the image transmission duration.

5SEC, 10SEC, 20SEC, 40SEC, 1MIN, 2MIN, 3MIN, 4MIN, 5MIN, 10MIN, 15MIN

###### CIf you selected “INTERVAL”, “ALARM IN1/2”, “MOTION”, or “ALARM OUT1/2” ...

In [INTERVAL], select the interval between e-mail transmissions.

1SEC, 2SEC, 3SEC, 5SEC, 10SEC, 30SEC, 1MIN, 3MIN, 5MIN, 10MIN, 15MIN, 30MIN, 1HOUR, 2HOUR, 3HOUR, 4HOUR, 5HOUR, 6HOUR, 8HOUR, 12HOUR, 24HOUR

The interval options available when you selected “ALARM IN1/2”, “MOTION”, or “ALARM OUT1/2” in [TRIGGER] are only “1SEC” to “15MIN”.

In [INTERVAL], the pull-down menu will only show options that do not exceed the [DURATION] setting.