Upgrade has been terminated.

Upgrade has been interrupted due to power off, network fault, or other problem during the process.

Redo the upgrade by proceeding as follows.

1Turn on the camera again.
2Access the camera again.
3Check the firmware version on [FIRMWARE UPDATE] in OPTION SETTINGS screen.
* If the version number is updated: Upgrade is complete.
* If the version number is not updated: Redo the upgrade.

The date and time is not adjusted automatically by the NTP server.

1The GATEWAY settings are not configured correctly.

Select NETWORK and configure the [GATEWAY] settings again.

2The NTP server address is not configured correctly.

Select CLOCK and configure the [NTP SERVER ADDRESS] settings again.

3Adjustment by NTP is not set as the method for automatic time adjustment.

Select CLOCK and set [CLOCK ADJUST] to [ON (NTP)].

The date and time information indicated on the live screen does not reflect the clock settings configured on the [CLOCK SETTINGS] screen.

It is recommended that you delete temporary Internet files.

To do so, in Internet Explorer, click [Internet Options] in the [Tools] menu and then delete temporary files, history, cookies, saved passwords, and web form information from the [General] tab.