You can install the following software on your PC to extend the capabilities of your surveillance system.

The CD-ROM that comes with the camera includes all the supplied software.

#### Supplied Software

###### AH.264 Plug-in (Plug-in for monitoring live video as high-quality moving images)

This plug-in software is required to display H.264 video on the live screen. Be sure to install it on each computer from which you access the camera via network operation.

###### BVA-SW3050Lite (Application for monitoring live video from more than one camera)

This monitoring application is designed for use with SANYO network cameras.

You can access up to 128 cameras simultaneously.

The application lets you monitor video images from connected cameras in either the single screen or the 4- screen, 9- screen, or 16-split screen mode.

###### CAuto IP Setup (Utility for automatically setting up IP addresses when two or more new cameras are connected)

This utility automatically assigns a unique IP address to each camera that has the factory default IP address (“192.168.0.2”).

Using the utility's camera search function, you can check the IP addresses of all cameras existing on the same local network.

It is also possible to check and correct overlapping IP addresses.

#### Optional Software

###### VA-SW3050Server/Client (Application for recording and playing back streaming images from camera)

This recorder/player application is designed for use with SANYO network cameras.

This is a complete version of the VA-SW3050 series software, which offers all the functions you need to perform monitoring, recording, search, playback, and other operations in a surveillance system.

This software requires at least two PCs that serve as the server and the client.