### Side Face

#### 1Auto Iris Lens Socket

Use this socket to connect an optional auto iris lens.

For details, refer to the “Lens Installation” section.

#### 2Operation Buttons

Use the buttons provided on the left-side face of the camera to perform the following operations.

These operations may be performed with the Web browser installed on your PC. For details, refer to the linked information.

Operation | Associated button and use | Equivalent network operation screen
--- | --- | ---
Restarting camera | Press the RESET button. | OPTION SETTINGS (CAMERA REBOOT)
Restoring factory default settings | Press the NEAR and SET buttons simultaneously. | OPTION SETTINGS (FACTORY DEFAULT)
Restoring factory default back focus position | Press the NEAR and FAR buttons simultaneously. | CAMERA SETTINGS (FOCUS ASSIST)
Resetting login password | Press the FAR and SET buttons simultaneously. | USER SETTINGS
Adjusting focus | For details, refer to the “Lens Adjustment” section. | CAMERA SETTINGS (FOCUS ASSIST/IRIS SETTINGS)
Adjusting iris
Viewing Firmware Version | For details, refer to the “Viewing Firmware Version” section. | OPTION SETTINGS (FIRMWARE UPDATE)

#### 3Bracket

This bracket may be attached to either the top or bottom face of the camera depending on the installation environment.

For bracket installation, be sure to use the longer screws supplied.

Install the camera securely to a durable location, taking into account the total weight of the camera mount (commercially available) and the camera.