Click CAMERA in the configuration menu to display the CAMERA SETTINGS screen.

The CAMERA SETTINGS screen includes a sub menu from which you can access 14 camera settings to configure the monitoring and other conditions of the camera.

Required operation privilege: admin, operator

#### Function of Each Screen Component

##### 1Sub Menu List

The CAMERA SETTINGS sub menu offers a list of camera settings.

1Sub menu: | Click one of the menu items in the sub menu to jump to the desired camera settings.
2 DEFAULT: | Click this button to reset all the settings you configured for the selected view (CAM1/CAM2) to the defaults (factory settings).

##### 2Configuration Section

This area shows a series of camera settings. You can use the vertical scroll bar and scroll buttons to scroll the settings up and down.

For each camera setting configuration section, the following buttons are provided.

1 SET: | Click this button when finished configuring the camera settings you accessed by clicking each sub menu item.
2 CANCEL: | Click this button before clicking SET to restore the previous settings.
3 DEFAULT: | Click this button to reset the settings on the camera configuration screen to the defaults (factory settings).
4HELP: | Click this to display a menu from which you can display the explanation of each configuration screen on the HELP screen.

###### Configuration Summary for Each Sub Menu Item

| Sub Menu | Operation | Application
--- | --- | --- | ---
1 | VIEW | You can have two patterns of view settings (CAM1/CAM2) by configuring the monitoring conditions through sub menu items “2 IRIS” to “11 PRIVACY MASK”. | VIEW
2 | IRIS | Configure the lens iris. | VIEW
3 | WHITE BALANCE | Adjust the white balance. | VIEW
4 | BLC | Configure the backlight compensation function. | VIEW
5 | SHUTTER | Configure the electronic shutter. | VIEW
6 | AGC | Configure the gain of the video signal. | VIEW
7 | DAY/NIGHT | Configure the Day/Night function that automatically switches the camera between color and black-and-white video modes depending on the luminance of the target. (This function is supported only by VCC-HD2300P/VCC-HD2300) | VIEW
8 | APERTURE | Configure the contour compensation function. | VIEW
9 | VIVID COLOR EFFECT | Configure the color saturation compensation function. | VIEW
10 | GAMMA | Configure the gamma correction level. | VIEW
11 | DNR | Configure the noise reduction function. | VIEW
12 | FOCUS ASSIST | Configure the focus assist function to adjust the focus. | Common
13 | MIRROR | Configure the mirror function to flip the subject on the monitor. | Common
14 | PRIVACY MASK | Configure the privacy mask settings to mask portions of the subject you want to hide for privacy protection. | Common

“Application” in the above table means the following:

VIEW: The configured settings will be applied to “CAM1” or “CAM2”, whichever you selected under [VIEW].

Common: The configured settings will be applied commonly to “CAM1” and “CAM2” selected under [VIEW].

##### 3Live Image Display Area

You can view how your changes affect the video image in real time.