Click CODEC/STREAMING in the configuration menu to display the CODEC/STREAMING SETTINGS screen.

Configure the conditions of the video/image transmission.

AConfiguring Aspect Ratio

BConfiguring JPEG images

CConfiguring H.264 video

Required operation privilege: admin, operator

If [SSL] is set to “ON” on the NETWORK SETTINGS screen, you cannot configure H.264 video.

### AConfiguring Aspect Ratio

###### In [ASPECT RATIO], select the aspect ratio (width-to-height ratio) of the video/image by clicking the corresponding radio button and click SET.

16:9 (Landscape), 4:3 (Portrait)

Clicking SET reboots the camera.

### BConfiguring JPEG images

1Configure the resolution (RESOLUTION).

The available options vary depending on your selection in [ASPECT RATIO].

16:9: 1920×1080, 1280×720, 1024×576, 640×360

4:3: 2288×1712, 1600×1200, 1280×960, 1024×768, 800×600, 640×480, 320×240

2Configure the image quality (PICTURE QUALITY).

BASIC, NORMAL, ENHANCED, FINE, SUPER FINE

3Configure the live video frame rate (LIVE FRAME RATE) for each operation privilege and click SET.

The available options vary depending on the model used.

VCC-HD2300/VCC-HD2100: 0.1ips, 0.2ips, 0.5ips, 1ips, 3ips, 5ips, 10ips, 15ips, 30ips

VCC-HD2300P/VCC-HD2100P: 0.1ips, 0.2ips, 0.5ips, 1ips, 2.5ips, 5ips, 8ips, 12.5ips, 25ips

Depending on the configured resolution, the available options for image quality and frame rate may be limited.

### CConfiguring H.264 video

1Configure the resolution (RESOLUTION).

The available options vary depending on your selection in [ASPECT RATIO].

16:9: 1920×1080, 1280×720, 640×360, 320×180

4:3: 1600×1200, 1280×960, 1024×768, 640×480, 320×240

2In [PRIORITY], select whether you put priority on the video/image quality or the bit rate.

QUALITY, BITRATE

###### When your selection in [PRIORITY] is “QUALITY” (PICTURE QUALITY)

Then, the system shows an appropriate bit rate depending on the selected quality.

BASIC, NORMAL, ENHANCED, FINE, SUPER FINE

###### When your selection in [PRIORITY] is “BITRATE” (BITRATE)

Type the bit rate directly, if you want to change it.

3In [FRAME RATE], select the frame rate of the stream.

The available options vary depending on the model used.

VCC-HD2300/VCC-HD2100: 15ips, 30ips

VCC-HD2300P/VCC-HD2100P: 12.5ips, 25ips

Depending on the configured resolution, the available options for image quality and frame rate may be limited.

4Select the H.264 video streaming method (PROTOCOL) and click SET.

UDP (Unicast), RTSP, HTTP, MULTICAST