Click OPTION in the configuration menu to display the OPTION SETTINGS screen.

On this screen, you can perform system-related operations and log checks.

Click SET to execute or start the intended operation.

Required operation privilege: admin, operator1

#### Rebooting Camera (CAMERA REBOOT)

If the camera stops functioning for some reason or other, in [CAMERA REBOOT], click SET to reboot the camera system.

#### Updating Firmware Version (FIRMWARE UPDATE)

You can update the camera's firmware to the latest version.

###### 1Click SET.

The FIRMWARE UPDATE screen appears.

###### 2Click BROWSE and select the firmware updater file.

###### 3Click EXECUTE.

The firmware update process starts. When the update process is completed, the camera system reboots and you reconnect to the camera automatically.

Once you reconnect to the camera, redisplay the OPTION SETTINGS screen and confirm that the firmware version has been updated.

Do not perform any operations on the screen or turn off the camera until the firmware update process is completed.

While the firmware is being updated, all camera functions stop working temporarily.

#### Restoring Factory Default Settings (FACTORY DEFAULT)

You can restore all the settings you have configured to the factory default settings.

###### In [NETWORK SETTINGS], select whether or not to restore the settings including the network settings and click SET.

WITH: Includes the network settings.

WITHOUT: Excludes the network settings.

An operation confirmation dialog box opens.

#### Backing Up Configured Settings (MENU BACKUP)

You can save the settings you have configured using the backup function.

###### In [MENU BACKUP], click SET. Then, select SAVE in a save confirmation dialog box and specify the backup destination file.

All the settings on the NETWORK SETTINGS screen and the [DATE/TIME] setting on the CLOCK SETTINGS screen are not saved.

#### Uploading Backed Up Settings (MENU UPLOAD)

You can restore the saved configuration settings of the camera from a backup file.

###### Click BROWSE, select the backup file you want to upload, and click SET.

The backup file is uploaded to the camera to restore the saved configuration settings.

When the upload process is completed, the camera system reboots.

All the settings on the NETWORK SETTINGS screen and the [DATE/TIME] setting on the CLOCK SETTINGS screen are not restored.

#### Viewing Logs (LOG)

Under [LOG], you can view the access and system logs.

You can click OUT PUT to output the content of each log into a text file.

The log information is deleted when the camera is powered off.

###### AACCESS LOG

Shows the history of access to the camera in chronological order (up to 100 entries).

Date and time, user name, authentication check result (OK/NG), connection destination IP address

###### BSYSTEM LOG

Shows a history of system operation in chronological order (up to 200 entries).