##### Camera

Image pickup device | 1/3" CMOS sensor
Effective pixels | 16:9 1920 (H) × 1080 (V), 4:3 2288 (H) × 1712 (V)
Lowest image illumination | 50IRE: 1.0 lx (at F1.2, color mode, high gain) 50IRE: 0.06 lx (at F1.2, black-and-white mode, high gain)
Video S/N ratio | 50dB (when AGC is “OFF”)
Lens mount | CS mount
Flange back adjustment | 12.5±0.5 mm, electrical flange back adjustment (Focus assist function)
Day/Night function | Auto, color, black-and-white, alarm input switching ( (VCC-HD2300P/VCC-HD2300 only))
White balance | Auto (ATW), one push (AWC), manual (R/B gain adjustable), indoor, outdoor, fluorescent
Backlight compensation | Multi-spot evaluative metering, center-weighted average metering, masking
Electronic sensitivity boosting | Auto (32× max) or Off
Electronic shutter | VCC-HD2300P/VCC-HD2100P: 1/25, 1/50, 1/120, 1/250, 1/500, 1/1000, 1/2000, 1/4000, 1/10000 VCC-HD2300/VCC-2100: 1/30, 1/60, 1/100, 1/250, 1/500, 1/1000, 1/2000, 1/4000, 1/10000 Long exposure shutter (1×, 2×, 4×, 8×, 16×, 32×)
Electronic iris | ON/OFF (Set [SHUTTER] to “EI”.)
Iris control | DC iris lens supported
Camera settings | Selectable between 2 camera setting patterns
AGC gain | Normal/Middle/High (Manual gain setting possible at Off)
Gamma correction | 0.45, 1, Mode 1, Mode 2
Aperture compensation | On/Off (Correction level adjustable)
VIVID COLOR EFFECT | ON/OFF
DNR | ON/OFF
Mirror | H/V/HV/OFF
Privacy mask | On/Off, max. 8 mask patterns
Motion sensor | On (masking/detection area setting)/Off
Language selection | English, French, German, Spanish, Japanese

##### I/O

Video output | Composite output
LAN | 10BASE-T/100BASE-TX (RJ-45 connector)
Alarm input | 2 (NO/NC), also serve as Day/Night switching signal (VCC-HD2300P/VCC-HD2300 only)
Alarm output | 2 (NO/NC, 16V, 150 mA, open collector)

##### Network

Image/video compression | H.264/JPEG
Video size (H.264) | (16:9) 1920×1080, 1280×720, 640×360, 320×180 (4:3) 1600×1200, 1280×960, 1024×768, 640×480, 320×240
Video size (JPEG) | (16:9)1920×1080, 1280×720, 1024×576, 640×360 (4:3) 2288×1712, 1600×1200, 1280×960, 1024×768, 800×600, 640×480, 320×240
Picture quality | QUALITY mode: BASIC, NORMAL, ENHANCED, FINE, SUPER FINE BITRATE mode: User-specified bit rate
Interface | 10BASE-T/100BASE-TX
Protocol | TCP/IP, UDP, HTTP, HTTPS, SMTP, NTP, DHCP, FTP, DDNS, RTP, RTSP, RTCP
Simultaneous access | 20
Security | BASIC authentication (ID/password), SSL, IP filtering

##### Others

Operating ambient temperature/humidity | –10 to +50°C, 90% RH or less (no condensation)
Power source | 12 to 15 VDC/24 VAC±10%, 50/60 Hz, PoE
Power consumption | 4,6 W
Weight | 220 g
Dimensions |

###### Accessories

1 Video cable

2 Cable holder for wiring

3 CD-ROM