### BFlange Back Adjustment

If you are using an optical zoom lens and zooming operation causes the camera to lose focus, adjust the flange back distance as follows.

1Press the SET button for 2 seconds or more.

The monitor now shows the SELECT MENU screen.

On the SELECT MENU screen, all information is displayed in English.

2Select [FOCUS ASSIST] using the NEAR/FAR button and press the SET button.

The monitor now shows the focus adjustment screen.

3Use the zoom and focus levers of the lens to focus on the subject at the telephoto end and press the NEAR/FAR button to adjust the focus.

Pressing the button causes the back focus position to change, which is indicated in the FB bar gauge (C).

The position changes step by step each time the button is pressed and continuously at a high speed when the button is held down.

4Use the zoom and focus levers of the lens to focus on the subject at the wide end and press the NEAR/FAR button to adjust the focus.

Repeat the above steps until switching between the telephoto and wide ends does not cause the camera to lose focus.

5Press the SET button for 2 seconds or more.

The focus adjustment screen will close.

The focus adjustment screen will also close automatically if left idle for 5 minutes or more.