I cannot set [SENSE UP] in [IRIS].

You cannot set [SENSE UP] when [SHUTTER] is set to “SHORT” or “LONG”.

Set [SHUTTER] to “OFF”.

I cannot set [SHUTTER] to “SHORT” or “LONG”.

You cannot configure the electronic shutter settings if you have set [SENSE UP] in [IRIS].

Set [SENSE UP] in [IRIS] to “OFF”.

I cannot turn off the AGC.

1If [DAY/NIGHT] is set to “AUTO”, you cannot set [AGC] to “OFF”. (When using VCC-HD2300P/VCC-HD2300)

Set [DAY/NIGHT] to “COLOR” or “B/W”.

2You cannot set [AGC] to “OFF” when [SENSE UP] in [IRIS] is set to “ON”.

Set [SENSE UP] in [IRIS] to “OFF”.