Click the desired button depending on the purpose of your operation. Then, the corresponding screen and panels will appear.

For details, refer to the linked information.

MENU: Click this to display the configuration menu.

LANGUAGE: Click this to display the language selection screen.

DISPLAY: Click this to display the display control panel.

### Displaying Configuration Menu (MENU)

Click MENU on the control panel to display the configuration menu that includes a series of menu selection buttons.

Clicking one of these menu selection buttons displays the corresponding configuration screen.

If you are a surveillance system administrator, use these buttons to configure necessary settings according to the installation environment and application of your camera.

Required operation privilege: admin, operator (“admin” only for NETWORK SETTINGS screen)

Without the required operation privilege, you will be presented with an authentication check dialog box when you click MENU on the live screen. In this case, you cannot access the menu selection buttons until you enter an adequate user name and password.

###### Menu Selection Buttons

| Button | Configuration Screen (Menu) | Operation
--- | --- | --- | ---
1 | NETWORK | NETWORK SETTINGS | Configure the network settings of the camera.
2 | CLOCK | CLOCK SETTINGS | Configure the clock date/time, daylight saving mode, automatic clock adjustment, and other settings.
3 | USER | USER SETTINGS | Configure the user authentication check at login.
4 | CODEC/STREAMING | CODEC/STREAMING SETTINGS | Configure the conditions of the video/image transmission.
5 | CAMERA | CAMERA SETTINGS | Configure the monitoring conditions and other settings according to the installation environment of the camera.
6 | ALARM | ALARM SETTINGS | Configure the alarm input/output settings and the motion sensor function.
7 | E-MAIL | E-MAIL SETTINGS | Configure the alarm notification e-mail function and other automatic transmission settings.
8 | FTP | FTP SETTINGS | Configure the image streaming conditions if you intend to record images from the camera to an FTP server.
9 | SECURITY | SECURITY SETTINGS | Configure the security settings for permitting or rejecting the access to the camera from up to 10 PCs.
10 | OPTION | OPTION SETTINGS | Perform operations such as updating the firmware, restoring the factory defaults, and backing up and uploading settings.

###### Other Buttons

| Operation Buttons | Function
--- | --- | ---
1 | HELP | Provides an explanation of each function.
2 | LIVE | Closes the configuration screen and returns to the live screen.