### CIris Adjustment (IRIS)

If the camera produces too dark, too bright, or other incorrect video images, adjust the lens iris.

1Press the SET button for 2 seconds or more.

The monitor now shows the SELECT MENU screen.

On the SELECT MENU screen, all information is displayed in English.

2Select [IRIS] using the NEAR/FAR button and press the SET button.

The monitor now shows the iris adjustment screen.

3Press the NEAR/FAR button to adjust the iris level.

The position changes step by step each time the button is pressed and continuously at a high speed when the button is held down.

NEAR: Closes the iris to produce darker images.

FAR: Opens the iris to produce brighter images.

4Press the SET button for 2 seconds or more.

The iris adjustment screen will be closed.

The iris adjustment screen will also close automatically if left idle for 5 minutes or more.