### BDetecting motion in specific areas

Use the motion detection function to detect motion in specific areas of the subject.

1On the ALARM SETTINGS screen, in [MOTION], select “DETECT”.
2In [DURATION], select how long you want the alarm state to be retained when the motion sensor detects motion and click DETAIL.

The detection area configuration screen appears.

5SEC, 10SEC, 15SEC, 20SEC, 30SEC, 45SEC, 1MIN, 2MIN, 3MIN, 4MIN, 5MIN

CC (Retains the alarm state as long as the motion alarm persists.)

The terminal will not accept subsequent alarm signals until the set duration expires.

The alarm state will be retained for at least 5 seconds even if the motion is instantaneous.

The configured duration value will be reset to the factory default value if you change any setting on the ALARM SETTINGS screen while an alarm state is retained.

To switch the alarm detection method, in [MOTION ALARM], click the desired radio button.

3Drag the mouse over live video/image to select the detection area.

You can set up to five detection areas.

Each detection area will be given a number (1 to 5) as you add it. The currently selected area is shown in yellow green.

To move a detection area, select it and then drag the mouse.

To resize a detection area, place the mouse pointer over its border and then drag the mouse.

To delete a set detection area, click the DELETE button (1) corresponding to the detection area number or drag it out of the screen.

4In [AREA], select the check box next to the area number of the area you want to enable.

You may select two or more check boxes.

5In [SENSITIVITY], select the detection sensitivity.

You can adjust the detection sensitivity to prevent unwanted detection.

The higher the value, the lower the sensitivity.

1 to 9

###### Checking how the motion sensor works

Click TEST (2).

If any motion is detected in a grid cell in the detection area, that cell will be shown in red.

Correct the detection conditions as required.

While the sensor is working, this button is labeled as END. To finish checking the motion sensor, click the button.

6Click SET and then BACK.

The settings are saved and you return to the ALARM SETTINGS screen.